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3U Gold-Plated Contacts

Model: RJ45-5ES

Main Features:
· [bookmark: OLE_LINK16][bookmark: OLE_LINK17]Durable design: ≥ 1250 mating cycles;
· Trident head ensures stable contact for rapid transmission;
· 3μin gold-plated contacts for optimized signal integrity.



	Connector Type
	　

	Category
	Cat 5e

	Type
	8P8C (Eight Position, Eight Contact)

	Shielding
	Shielded

	　
	　

	Material
	　

	Housing Material
	Polycarbonate

	Shielding Material
	Brass with nickel plating

	[bookmark: OLE_LINK8][bookmark: OLE_LINK9]Contact Material
	Copper

	Contact Surface Material
	Gold Plating on Nickel Barrier

	Gold Plating Thickness
	[bookmark: OLE_LINK4][bookmark: OLE_LINK6]3U (3μin or 0.0762 µm)

	　
	　

	Electrical Properties
	　

	Voltage/Current Rating
	125 VAC / 1.5 A

	Insulation Resistance
	≥ 500 MΩ

	Contact Resistance
	≤ 20 mΩ

	Dielectric Withstand Voltage
	1500 V DC/AC Peak

	　
	　

	Mechanical Properties
	　

	Durability
	≥ 1250 mating cycles

	Wire Gauge
	0.85 mm ≤ Ø ≤ 1.1 mm

	　


	　

	Environment
	　

	Operating Temperature
	-40°C to 70°C

	Operating Humidity
	RH 10% to 90% (non-condensing)

	Storage Temperature
	-40°C to 80°C

	Storage Humidity
	RH 5% to 96% (non-condensing)

	　
	　

	General
	　

	Dimension
	23x12x8 mm (LxWxH)

	Net Weight
	2.2 g

	　
	　

	Diagram
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